Test report

Motion planning design

Sampling based method

Simple trajectory generation


Path smoothing

Test on functionals


Trajectory tracking

This report offers the test result in trajectory generation functionals.


1. Lane changing functions test
2. Lane change trajectory generation test. We generate the four cases where we apply lane change functionals.
   1. Vehicle turning left, with lane changing left




* 1. Vehicle turning left, with lane changing right



* 1. Vehicle turning right, with lane changing left



* 1. Vehicle turning right, with lane changing right



1. Comparison between two different center line generation

We have two difference methods in generating a sequence of center line waypoints for future use. One is, based on current polynomials of lanes on the left and right, discretely sample on Cartesian coordinate along x axis to get the y axis value, and calculate its mean value. And the other method is discretely sample under Frenet coordinate, which means it integrate along s direction. At each sample point, get the respective x value on each lane polynomial. We provide both methods realization and make comparison numerically.

* 1. Using Cartesian coordinate to generate a sequence of center line waypoints.



* 1. Using Frenet coordinate to generate a sequence of center line waypoints.



As you can see in the figure, the upper triangle line is using Frenet method, while the blue dashed line is using Cartesian method. They almost overlapped. As for the calculation time, we also make a comparison as follows:

The prerequisite is that both methods generate a sequence of trajectory of 80m, and the sampling resolution is about 0.2m, which means about 400 points will be generated. The calculation time is (with CPU performance i7-9750H @2.60GHz and RAM 32G):

Using Cartesian method:

*reference\_1 generation time is: 1.680400 ms*

Using Frenet method:

*reference\_2 generation time is: 4.659700 ms*

1. Kappa calculation

In our module, we provide two difference kappa calculation methods, one is deducted by pure math, while the other uses discrete interpolation.


The first one use close form equation as follows:

The other method is as follows:

where

and

In the next few steps of path smoothing, we decided to trust the first method. And the two methods comparison is as follows:




1. Path smoothing method:


Since the original trajectory generated by Bezier curve cannot guarantee that the curve can satisfy the vehicle kinematic constraints, say, the max curvature constraints. Therefore, we designed a path smoother which aims to minimize 1) the distance between the origin reference line and the optimized trajectory. 2) the smoothness of the optimized trajectory.


In this smoother, we penalized the norm of the offset between reference line and optimized trajectory, and the norm of . The objective function is as follows:

We use gradient descent method (do derivative over ) to minimize objective function by iterative search.

We also add some stopping criteria to ensure the robustness of the method. The first term is constrained by add a maximum offset between the reference line and optimized trajectory, one the offset increases upper to the upper bound, the iteration will be forced to stop. In terms of curvature, we add a maximum curvature constraint as well. In each iteration, we will check the curvature of the optimized trajectory, once all the points on the trajectory satisfy the curvature limit, iteration will also be stopped. To fix the running time of the iterative search part, we lastly constrained the maximum iteration number as a constant. Several examples of the smoother performance are as follows, where we are smoothing the lane changing reference line, with lateral offset 3.5m, and longitudinal variation between 50m to 80m.







As for the calculation time added by smoothing module, we use a simple example to show the approximate running time. In this example, we smooth an original Bezier curve with lateral offset of 3.5m, and longitudinal distance of 50m, the smoothing parameter alpha is set as 0.01, and beta 0.7, the running time is 62.135 *ms*, and the iteration loop number is 124.

1. Sampling method

In this section, we want to discuss how we use sampling-based method in our design. This section is organized as follows: 1) we discuss difference rules in do sampling-based planning. 2) we divide on-road planner scenario by scenarios and introduce different sampling method in dealing with these scenarios. 3) we specifically discuss how to use sampling method. 4) we introduce a simplified trajectory generation method to help realize Lane Changing Assistant (LCA). 5) we discuss how to make sampling more efficient. 6) we discuss how to choose cost function terms.

1). Difference sampling rules

In sampling-based method, we should always obey the rule that we combine two dimensions at a time. For example, we can sample x(t) and y(t) and combine them together to get spatial-temporal profile. By doing derivative over time the velocity profile can also be generated. Another method is to sample y(x), and x(t), which we named more formally as “SL and ST graph”. The y(x) is the SL graph, which indicates the relationship between lateral position and longitudinal position. The x(t) is the ST graph, which indicates the relationship between longitudinal position s and time t. In terms of sampling dimensions, SL samples on lateral offset L and longitudinal S, and ST samples on time T and longitudinal S. The specific methods will be discussed later.

Another sampling method, as mention above, is to sample lateral offset x and time t, and longitudinal s and time t, say x(t) and y(t). let us compare between these two sampling methods. As for the first method, SL and ST graph method, can be applied more specific kinodynamic constraints (which mean considering vehicle kinematics and dynamics). The reason is that we can calculate on SL graph the curve curvature, jerk (spatial continuity), etc. while in its counterpart, x(t)-y(t) sampling method, we only have separately spatial temporal profile laterally and longitudinally, which means it is more decoupled in the two directions, therefore we are less likely to apply kinodynamic constraints on the curve. The only thing we can do is to check it feasibility at the very end of the trajectory generation process. More specifically, we can only do velocity, acceleration, and curvature check when the two graphs are combined to together. Since feasible velocity and acceleration in each direction does not guarantee that they are feasible after combining. And curve curvature cannot be calculated until combining. This method, however, also has its merits. Since it is sampled in lateral and longitudinal over t, it is more sensitive to deal with dynamic obstacles, for example, merging situation. When we have time information in both dimensions, sampling can be more organized. We can have unified T sampling range for both x(t) and y(t), since the two directions are decoupled. Even though SL-ST method samples time in ST graph, but since we have longitudinal sampling in SL graph, for different sample S, we have to first calculate a feasible T duration, so that it can be realized longitudinally. Therefore, In ST graph sampling of T, it is more uncertain. Uncertainty always decrease robustness. The advantages of x(t)-y(t) method is obvious, while its weakness, as mentioned, is also obvious: decoupling lateral and longitudinal sampling means neglecting vehicle kinodynamics. Postponing status checking which ensures trajectory feasibility always leads to low efficiency. As you need to check on each candidate curve for its feasibility, and calculation efforts are wasted until you find the sub-sub-…sub-optimal trajectory that satisfy the status checking.

2) therefore, we decide to divide our target scenarios into several classes so that we use difference sampling methods to enlarge their advantages at most.




Fig. x: We divide the on-road driving into several scenarios, and in each scenario, the motion planner can be slightly different.

1. Lane following

This scenario deals with only lane following without lane changing, it is further separated into velocity following and distance following. Since this is the simplest scenario, we want to simplify planning process as much as possible, even in longitudinally planning, we give up sampling method. Instead, we use trajectory tracking method longitudinally, with reference line (usually rough lane centerline is provided by mapping module, and post-processed by smoother module). Such decide at most reuse the merits of LKA and ACC functionals.

1. Stopping

As for stopping scenarios, for example, stopping in front of the red traffic lights, or in front of some static obstacles appearing in front of the lane, etc. we create a virtual stopping line where the vehicle must stop to deal with this scenario. Laterally, we still use the same method as lane following, assuming that we will not allow sudden steering when the vehicle is in process of stopping. Longitudinally, we apply s(t) method, where we sample on longitudinal distance s and time t, to get a profile. By doing derivative over time, we get relationship between longitudinal distance s and time t.

1. Lane changing

Even for lane changing scenarios, we still divide it into several more specific situations, say, lane changing whose target lane is still its original lane (temporarily changing its lane, for example avoiding a static or dynamic obstacle in front of ego vehicle’s current lane, truck avoiding, etc.) and lane changing whose target lane is some adjacent lane (permanently changing its lane, for example manual lane changing, automatic lane changing, merging, etc.).

For the first situation, we apply SL-ST method. Since we do not have too much velocity interaction with other vehicles. The most important issue in dealing with such scenarios is lateral planning, we still can use original ACC functional to support its longitudinal velocity planning, as we do not care too much about at what exact timestamp, we reach the lateral position. We only care about that the vehicle can at some time during go through the lateral positions as we have previously planning. In dealing with static and dynamic obstacles, and temporarily shifting the reference line a little bit to avoid adjacent trucks, such method works well. In terms of computational efforts, this method only sample in longitudinal s and time t, which means it decreases the sampling dimension from 3 to 2, greatly reduce the computational efforts. ACC and LKA always uses less computational effort that sampling based method; thus, our principle is that we use ACC and LKA so long as the scenario is simple enough to support such functional combination.

For the second situation, where vehicle permanently change its lane, we also divide it into two different situations. For simple lane changing, we plan laterally using SL graph, and ACC plans longitudinal velocity. While for merging situation, which is the most complex so far, we use x(t)-y(t) method. You may feel that we can still use SL-ST method in such situation, but the answer is NO. Imaging that we need to cut into the middle position of two adjacent vehicles. We have to calculate the exact which is a function of t, and if we first planning the SL graph where we get d(s) (d is lateral offset), actually, we have fixed the time t. If we sample on t, the varies, but in ST graph, we want to sample on both S and T. As mentioned, we have fixed t in SL sampling, we do not have any freedom in sampling on t in ST graph. To sum up, in dealing with merging situations, if we try to use ST-SL method, one dimension is always fixed due to their coupling relationship.




Fig. x: In merging scenario, one dimension is always fixed due to the coupled relationship between the three dimensions.

Now it is obvious that x(t)-y(t) method is the only choice we have in dealing with merging. We first sample on d (lateral offset), and then sample on T, once T is determined, we have , the longitudinal s sampling is around the . In this method, the three parameters, x, y, t is three free dimensions, and no dimension is fixed due to their coupled relationship.

3) algorithms of planning in different scenarios

a). Lane Following

b). Stopping

c). Avoiding Static Obstacles

d). Avoiding Dynamic Obstacles

e). Avoiding Truck

f). Simple Lane Change for LCA

g). Simple Automatic Lane Change

H). Merging

The most complex on-road scenario in this report is merging, as we consider both longitudinal and lateral planning at the same time. In other cases, we can simplify scenarios to decrease sampling dimensions from 3 to 2. In this case, however, it seems that we cannot avoid sample on all three dimensions at the same time. As for choice of sampling method, as mentioned in previous section, we must use x(t)-y(t) method. Based on [Werling,2010], we apply very similar merge scenario sampling.

In lateral movement design, we plan x(t) under instantaneous vehicle coordinate. Human perception obviously weights lateral and longitudinal changes of acceleration differently. We introduce jerk in both longitudinal and lateral directions in Frenet coordinates, which are denoted by and . From [xxx] we know that quintic polynomials are the jerk-optimal connection between a start state = [, , ], and an end state = [, , ] within the time interval T in a one dimensional problem. More precisely, they minimize the cost functional given by the time integral of the square of jerk

Since we seek to minimize the squared jerk of the resulting trajectory, we choose the start state of our optimization = [,, ] according to the previously calculated trajectory ***s***, so that no discontinuities occur. For the optimization itself, we let  *= = 0*, as we always want to constrain the terminal states, which is lateral velocity and lateral acceleration, to zero. In addition, we choose and end state lateral offset d as another two cost function penalty items. The cost function is denoted by:

,

where ,, and is respective penalty weights on different parameters. is the mean value along the planned trajectory, T is planning time T, and is mean value of squared lateral offset of the planned trajectory along the reference line.

Instead of calculating the best trajectory explicitly and modifying the coefficients to get a calid alternative, we generate in the first step a whole trajectory set: by combining different end conditions:

*=* []*,*

where we sample on end state of lateral offset ***d***, and planning time ***T***. as we have mentioned in previous section that x(t)-y(t) method does not support curvature calculation, therefore, we only choose three penalty items in cost function. Status checking such as velocity checking, acceleration checking, curvature checking, and collision checking have to be postponed until we generate respective longitudinal trajectory x(t). after we combine the x(t) and y(t) trajectory and get the trajectory with lowest cost function, we check the trajectory against velocity, acceleration, curvature, and collision. If we are luck, it is valid, and we are done. If it is not, we would have to pick up a “sub-optimal” trajectory with the second lowest cost function, and do status checking again until we find a collision free alternative.

In this section, we discuss our method of candidate trajectory generation method which is based on lattice sampling (kind of), notice that we do not precompute the lattice heap matrix. In our functionals, this is realized and simulated in frenet\_Bezier\_Sampling.m file, and we also provide a simpler functional where a Bezier curve is individually generated once for Lane Change Assistant (LCA) use which is realized and simulated in frenet\_Bezier\_simpleRule.m.

We divide our on-road planner scenario by scenario, more specifically, merging, velocity keeping, following, and stopping.

1. Bezier curve sampling method
2. Quintic polynomial sampling method
   1. lateral trajectory planning
   2. Longitudinal trajectory planning

In this section, we……

Following is a test on the robustness of using quintic polynomial to do longitudinal trajectory planning. The test file named as *test\_on\_long\_poly.m* is the simulation code for testing such polynomial in longitudinal direction. By changing the fixed boundary conditions, we can plot the longitudinal profile of x(t), v(t). combining these two figures together, we can get s(v), and when spatial-temporal profile is given, we can search respective v at specific s in the s(v) graph. As we mentioned above, we do not use such method in dealing with merging tasks, but it works well in other scenarios.


We use the file to do a simple test in test\_on\_laneChanging.slx. The assumption for this test is as follows: we have two adjacent lane vehicles on the right-hand side moving at the same speed as ego vehicle, which is 30 kph. The ego vehicle has the same longitudinal distance as the first neighbor vehicle that is closest to ego vehicle, and the other vehicle is about 50 meters ahead of the first neighbor car. The test scenario is that the ego vehicle is going to merge into the area between the two neighbor vehicles. This test file can generate a speed profile alongside the longitudinal *s*, and it can be used in *test\_on\_laneChanging.slx* file for Carmaker simulation. This test file has not added sampling-based method longitudinal planning functionals and it also does not support such functional simulation. Therefore, it can only test on very specific situation, say, fixed boundary conditions. The merits of this test file are a brief view of how quintic polynomials performs in longitudinal planning and have a look at the changing lane functional performance. Later, when sampling-based functionals are developed, the sampling strategies can also be tested under the similar framework.

The result of this test file is shown in the following figures.





In merging scenarios, the most important thing is velocity control, therefore, a precise velocity tracking controller is critical, it can greatly affect the system performance in merging maneuvers. The following figure is the velocity and steering angle during the merging process. We can see that the ego vehicle velocity increase first and then decrease. Since we only have a simple test with boundary condition fixed, we can not penalize high acceleration during merge, actually, we do not have any control on the duration acceleration. That is why we need to introduce sampling-based method so that we can penalize high acceleration through sampling and cost function minimization.



[ ] Werling M, Ziegler J, Kammel S, et al. Optimal trajectory generation for dynamic street scenarios in a frenet frame[C]//2010 IEEE International Conference on Robotics and Automation. IEEE, 2010: 987-993.